| **Raw Material** | **Amount stored** | **How is it stored?** | **Storage Location** | **Purpose** | **Annual Usage (kg)** |
| --- | --- | --- | --- | --- | --- |
| CRESYLIC RESIN WAC 2 RMS 232 | 2403.20 l | IBC | Chiller | Filament Winding | 18000 |
| Cellobond SC1008P | 1,500 kg | 215kgs drum | Chiller | Wide Width | 60000 |
| Methylated Spirits | 1000 | DRUM FULL SIZE | Flammable store | Wide Width | 4000 |
| Phenolic Resin | 5000 l | IBC | Flammable store | Wide Width | 97853 |
| Phenolic Resin | 5000 l | IBC | Flammable store | Wide Width | 86635 |
| Polyester Resin | 6600 l | IBC | Flammable store | Wide Width | 130205 |
| EPOXY RESIN RMS 307 | 2296.32 | Drum | Resin Compound | Filament Winding | 4180 |
| EPOXY ANHYDRIDE CURING AGENT RMS 308 | 1776.84 | Drum | Resin Compound | Filament Winding | 3740 |
| Phenolic resin for Paper impregnation Bitrez grade Curaphen 46-358 M58 to raw material specification TRMS3014 Issue 2 | 10 x 1,000kg IBC | IBC | Resin Compound | Wide Width | 29000 |
| Phenolic Resin for Fabric I to our Raw material specification TRMS3015 Issue 1mpregnation (Mathanol) Bitrez grade Curaphen 46-362 M60 | 10 x 1,000kg IBC | IBC | Resin Compound | Wide Width | 48680 |
| Araldite ® Z 7062 N75 Resin to our raw Material Specification 4001 | 4 x 200kg Drums | Drum | Resin Compound | Wide Width | 4800 |
| Melamine Resin EML 110 to our Raw Material Specification TRMS 4506 Issue 011 | 1,200kg | 1 x IBC | Resin Compound | Wide Width | 2400 |
| SEE RM4511 Epoxy Resin MY750 to be supplied in accordance with our raw material specification TRMS 4510 alternatively Epoxy Resin NPEL128n to be supplied in accordance with our raw material specification TRMS 4511 | 4 x 240kg Drums | Drum | Resin Compound | Wide Width | 6720 |
| Industrial Methylated Spirits 94 to our Raw Material Specification TRMS 5600 issue 009 | 8 x 170kg Drums | Drum | Resin Compound | Wide Width | 1360 |
| Acetone to our Raw Material Specification TRMS 5601 Issue 010 | 8 x 165kg Drum | Drum | Resin Compound | Wide Width | 5980 |
| DiMethyl Formamide to our Raw Material Specification TRMS 5605 Issue 9 | 4 x 200kg Drums | Drum | Resin Compound | Wide Width | 2400 |
| Acetone | 1810 | Drum | Resin Compound | Wide Width | 12880 |
| IDA (INDUSTRIAL DENATURED ALCOHOL) | 9110 kg | 165kgs drum | Resin Compound | Wide Width | 40000 |
| Araldite ® LZ7062 | 3860 | Drum | Resin Compound | Wide Width | 6000 |
| Araldite ® Z8001 or XTW 9820 A80 | 1,000 | Drum | Resin Compound | Wide Width | 1000 |
| Methyl Cellusolve/ Methyl Glycol | 8895 | Drum | Resin Compound | Wide Width | 10140 |
| MY750 | 560 | Drum | Resin Compound | Wide Width | 40000 |
| HYPERLAST EMH 85A Prepolymer | 400 | Drum | Resin Compound | Paint/Spray | 1320 |
| White Diesel | 280 litres | 280 litre drum | Resin Compound | Fuel for sprinkler system |  |
| Hydraulic oil | 8000 litres | IBC's, 280 litre drums or 20 litre pails | Resin Compound |  |  |